Open topic with navigation

# Configure Connector Framework Server

This section describes how to configure CFS.

To configure CFS

1. Stop CFS, if it is running.
2. Open the CFS configuration file.

3. In the `[Service]` section, specify the service information, for example:

   `ServicePort` | The port for CFS to use as the service port.

4. In the `[Server]` section, set the following parameters:

   `Port` | The port for CFS to use as the ACI port.
   `AdminClients` | The host names, or IP addresses, of machines that are permitted to send administrative commands to the CFS.
   `QueryClients` | The host names, or IP addresses, of machines that are permitted to send queries to the CFS ACI port.

5. (Optional) In the `[ImportService]` section, you can set parameters to configure KeyView. You can choose the number of threads to use, specify the folders to use for extracting files, and customize how documents are imported.

   `ThreadCount` | The number of threads to use for importing documents.

   For information about the configuration parameters that you can set, refer to the Connector Framework Server Reference.

6. Save the configuration file.

Related Topics

- Start and Stop Connector Framework Server
- Connector Framework Server Configuration File
- Customize Logging

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm