Open topic with navigation

# PortN

The `PortN` parameter specifies the ACI port of the Distributed Connector. Set this parameter to the port specified by the `Port` parameter in the `[Server]` section of the Distributed Connector configuration file. You can register a connector with more than one Distributed Connector.

Type: | Integer
Default: | 10000
Required: | No
Configuration Section: | DistributedConnector
Example: | `Port0=10000`
See Also: | HostN DataPortN ConnectorGroup

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm