Open topic with navigation

# MaxKBPS

Use this parameter to specify the maximum bandwidth in kilobytes per second a spider can use at any time. Enter 2000000000 if you do not want to restrict the amount of data.

Type: | Long
Default: | 4096
Required: | No
Allowed Range: | Minimum: 0 Maximum: 2000000000
Recommended Range: | Minimum: 1 Maximum: 64
Configuration Section: | TaskName or Default
Example: | `MaxKBPS=128`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm