Open topic with navigation

# ServicePort

The port on the host server on which the service listens for service status and control requests.

Type: | Long
Default: | 40010
Required: | Yes
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1024 Maximum: 65535
Configuration Section: | Service
Example: | `ServicePort=40010`
See Also: | ServiceACIMode ServiceControlClients ServiceHost ServiceStatusClients

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm