Open topic with navigation

# DIHEngine`N` Configuration

In the `[DIHEngines]` section you must create a `[DIHEngineN]` subsection for each IDOL server to which the Distributed Index Handler sends index actions. Each `[DIHEngineN]` subsection specifies the host and ACI port of a child IDOL server.

Note: You must number child IDOL server sections in consecutive order, starting from 0 (zero).

For example:

    [DIHEngines]
    Number=2

    [DIHEngine0]
    Host=localhost
    Port=9000

    [DIHEngine1]
    Host=12.3.4.56
    Port=9000

DistributeByFieldsValues
Host
Polling
Port
UpdateOnly
ServiceSSLConfig
SSLConfig

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm