Open topic with navigation

# PeriodInSec

The time in seconds dedicated for indexing data on each child server, after the first roll over has occurred. At the end of this period, a DREINITIAL index action is sent to the next child server and ACI requests are sent to the DAH to power up or power down the appropriate child server.

If you do not use this parameter, then you must use PeriodInDay to set a period.

Type: | Long
Default: |
Required: | No
Configuration Section: | RoundRobinMode
Example: | `PeriodInSec=86400`
See Also: | PeriodInDay

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm