Open topic with navigation

# [ACIEncryption] Section

You can encrypt communications between ACI servers and applications that use the HPE ACI API by configuring an `[ACIEncryption]` section in each of the application configuration files. For example:

    [ACIEncryption]
    CommsAllowUnencrypted=False
    CommsEncryptionType=GSS
    ServiceName=kerberos

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm