Open topic with navigation

# [DistributionIDOLServers] Section

When you run the DAH and DIH in a unified IDOL Server configuration, use the `[DistributionIDOLServers]` section to set the total number of IDOL Servers with which the DAH and DIH communicate. Child servers defined in this section handle both ACI actions and index actions. For more information refer to the Distributed Action Handler Administration Guide and the Distributed Index Handler Administration Guide.

You must create an `[IDOLServerN]` subsection for each of the IDOL Servers or other child servers that the DAH and DIH communicate with, in which you can specify the server configuration details.

    [DistributionIDOLServers]
    Number=2

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm