Open topic with navigation

# [DIHEngines] Section

When you run the DIH in a unified IDOL Server configuration, you can configure child servers for DAH and DIH separately. This process allows you increased flexibility when querying and indexing content in remote servers. For example, you can configure different child servers to perform indexing or actions exclusively. For more information, refer to the Distributed Index Handler Administration Guide.

Use the `[DIHEngines]` section to set the total number of IDOL Servers that the DIH sends index actions to.

You must create a `[DIHEngineN]` subsection for each of the child servers that the DIH sends index actions to. In these sections you specify the server configuration details.

For example:

    [DIHEngines]
    Number=2

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm