Open topic with navigation

# ServiceStatusClients

The IP addresses or names of clients that can request status information from a service. Separate multiple individual addresses with commas. There must be no space before or after the comma.

Adding a client to `ServiceStatusClients` does not enable it to send service control actions. To enable a client to send service control actions, you must add the IP address or host name to the ServiceControlClients.

You can use wildcards in the IP addresses. For example, type `187.*.*.*` to permit any machine whose IP address begins with `187` to access the service's status. You can also filter the `ServiceStatusClients` parameter using CIDR notation.

Type: | String
Default: | None
Required: | Yes
Configuration Section: | Service
Example: | `ServiceStatusClients=localhost,127.0.0.1`
See Also: | ServiceACIMode ServiceControlClients ServiceHost ServicePort

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm