Open topic with navigation

# And Engine Configuration Parameters

An And engine compares two tracks to identify events in the second track that occur within a specific time interval of events in the first track (before and/or after the first track's event). The engine produces a track containing the identified record pairs. This section describes the parameters that you can set in the configuration section for an And ESP task.

Configuration Parameter | Description
--- | ---
Input0 | The first input track.
Input1 | The second input track.
LuaScript | The path of a Lua script that defines conditions that a record pair must meet in order to be included in the output track.
MaxTimeInterval | The maximum interval from a record in the first track to a record in the second track, for the two records to be considered a pair.
MinTimeInterval | The minimum interval from a record in the first track to a record in the second track, for the two records to be considered a pair.
Type | The type of ESP engine to use. Set this parameter to `And`.

## Output Tracks

This engine produces a single output track, named `TaskName.Output`.

Field name | Type | Description
--- | --- | ---
`record0` | Record | The record from the first input track (Input0)
`record1` | Record | The record from the second input track (Input1)

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm