Open topic with navigation

# BarcodeTypes

A comma-separated list of the types of barcodes that might appear in the ingested media. The following types are available:

Codabar | IATA 2/5
Code-128 | Industrial 2/5
Code-39 | Matrix 2/5
Code-93 | Patch Code
Datalogic 2/5 | PDF417
Data Matrix | QR
EAN-13 | UPC-A
EAN-8 | UPC-E
I25 |

Note: UPC-A is a subset of EAN-13. Setting `BarcodeTypes=EAN-13` means that Media Server will return all EAN-13 barcodes including UPC-A.

Note: ISBN barcodes are a subset of EAN-13 that begin with 978 or 979, so you can detect ISBN barcodes by setting `BarcodeTypes=EAN-13`, but Media Server will also return EAN-13 barcodes than are not in the ISBN range. Similarly, you can detect GS1-128 barcodes (sometimes known as UCC/EAN-128) by setting `BarcodeTypes=Code-128`, because these are a subset of Code-128 barcodes.

Alternatively, you can set one of the following values to process multiple barcode types:

`All` | All supported types.
`All1D` | All one-dimensional types.
`All2D` | All two-dimensional types.

Type: | String (comma-separated list)
Default: | All
Required: | No
Configuration Section: | TaskName
Example: | `BarcodeTypes=QR`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm