Open topic with navigation

# MinPhoneRate

The minimum phone rate (phones per second) that a segment must have in order to be considered valid.

Action: | AddTask
Task: | LangIdSegWav, LangIdCumWav, LangIdBndWav, LangIdSegStream, LangIdCumStream, LangIdBndStream, LangIdSegLif, LangIdCumLif, LangIdBndLif
Type: | Integer
Default: | 1.0
Example: | `MinPhoneRate=1.0`
See Also: | MinPhoneRate (configuration parameter)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm