Open topic with navigation

# AmFile

The acoustic model file to use.

For the amadaptadddata module, the acoustic model is used as a base when running acoustic adaptation.

For the [dataobfuscation] Module Configuration, the acoustic model is used to produce the obfuscated training data.

For the `myResource` configuration sections, the acoustic model replaces the language pack's default acoustic model.

*You must set the value of this configuration parameter by setting the corresponding action parameter.

You can specify an absolute or relative file path. If you specify a relative path, it is considered as being relative to the acoustic model directory. If the file path is excluded, IDOL Speech Server defaults to the acoustic model directory.

Note: The TrainedAmDir parameter in the `[Paths]` section of the configuration file sets the location of the acoustic model directory.

Type: | String
Default: | None
Required: | Yes
Configuration Section: | amadaptadddata module, dataobfuscation module, and MyResource (language packs only)
Example: | `AmFile=T:\LP\ENUK\ver-ENUK-5.0-16k.am`
See also: | Am (action parameter for `amadaptadddata` and `dataobfuscation` modules) TrainedAm (action parameter for `myResource` configuration sections)

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm