Open topic with navigation

# Al_MaxPeriod

The `Al_MaxPeriod` parameter specifies the end of the autocorrelate period range after the current start time, in seconds.

Type: | Decimal
Default: | 2.0
Range: | 0.5–5.0
Required: | No
Configuration Section: | audiosec module
Example: | `Al_MaxPeriod=2.0`

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm