Open topic with navigation

# Gb_EdgeTrigger

The `Gb_EdgeTrigger` parameter specifies the glass break edge trigger threshold for detecting the initial impact.

Type: | Decimal
Default: | 2.0
Range: | 1.0–32.0 0.0 disables the parameter.
Required: | No
Configuration Section: | audiosec module
Example: | `Gb_EdgeTrigger=2.0`

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm