# TPVAPITextInfo

## Description

This structure defines a text buffer. See VAPINM_TEXTBUFFER.

## Syntax

    #include <kvvapi.h>
    typedef struct tag_TPVAPITextInfo
    {
        long        lBaseAddress;
        int         cbText;
        BYTE*       lpText;
    }
    TPVAPITextInfo;

## Members

`lBaseAddress` | A long integer that returns the base logical address at the start of the buffer.
`cbText` | An integer that returns the number of bytes in the buffer.
`lpText` | A pointer to the byte buffer, which returns the pointer to the text buffer. The text buffer can contain text or commands. Commands are ANSI strings with the following extensions (embedded control codes): `KV_EOP 0x01` End of paragraph. `KV_EOC 0x02` End of cell. `KV_PIC 0x03` Picture exists at this logical address.

© Copyright 2016-2020 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm