Open topic with navigation

# ModeValue

Sets the value of the parameter associated with the speech-to-text algorithm mode specified by the Mode parameter.

Setting `ModeValue` high increases the accuracy of the analysis.

- If `Mode=fixed`, the `ModeValue` is the beam width of the search process. A higher beam width than the default leads to slower but possibly more accurate processing, while a lower beam width is faster but probably less accurate.

- If `Mode=relative`, the `ModeValue` corresponds to real-time scaling. The higher the value, the longer processing takes.

- If `Mode=live`, `ModeValue` has no effect.

Action: | AddTask, CheckResources
Task: | AfpAddTrackStream, LangIdBndStream, LangIdCumStream, LangIdSegStream, StreamSidOptimize, StreamSidTrain, StreamSpeakerId, StreamToText, TelWavToText, WavToTextPunct, TelWavToTextPunct, StreamToTextPunct
Type: | String
Default: |
Example: | `ModeValue=4.0`
See also: | ModeValue (configuration parameter) Mode

© 2014 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm